<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<library>
<description>&lt;b&gt;Raspberry Pi&lt;/b&gt; by &lt;b&gt;Martin's Bastelstube&lt;/b&gt;
&lt;p&gt;
Different shapes of piggyback boards for the famous &amp;amp; fabulous
&lt;a href="http://www.raspberrypi.org/"&gt;Raspberry Pi&lt;/a&gt; computer.
&lt;p&gt;
The outline of the Raspberry Pi board is drawn on layer 52 bDocu, so you can make it invisible if necessary.&lt;br/&gt;
Recommendation: Start your design with RASPI_BOARD_FULL, so you are aware of all the big components and
connectors when you're drawing the dimensions of your board and placing your own components.&lt;br/&gt;
Later, you can simply change the package of your Raspberry Pi connector to the RASPI_BOARD_EDGES type,
so you can concentrate on your own design.

&lt;hr&gt;&lt;br/&gt;

Designed by &lt;a href="http://bastelstube.rocci.net/"&gt;Martin's Bastelstube&lt;/a&gt;&lt;br&gt;
Comments / complaints / bug reports / suggestions to &lt;author&gt;eightbit@web.de&lt;/author&gt;</description>
<packages>
<package name="RASPI_GPIO_PIN">
<description>26-pin connector for Raspberry Pi GPIO&lt;br/&gt;
 &amp;nbsp; just the two rows of pins</description>
</package>
<package name="RASPI_BOARD_EDGES_2DRILL">
<description>Raspberry Pi board, outline is only marked by its edges&lt;br&gt;
including 2 drill holes for Model B Revision 2.0</description>
</package>
<package name="RASPI_BOARD_FULL">
<description>Raspberry Pi board, full outline with position of big connectors + components&lt;br&gt;
including drill holes for Model B Revision 2.0</description>
</package>
<package name="RASPI_BOARD_EDGES_1DRILL">
<description>Raspberry Pi board, outline is only marked by its edges&lt;br&gt;
including 1 drill hole for Model B Revision 2.0</description>
</package>
<package name="RASPI_BOARD_THIN_DRILL">
<description>Raspberry Pi board
 - 
Thin version with only the width of the GPIO connector and 1 drill hole</description>
</package>
<package name="RASPI_GPIO_BOX">
<description>26-pin box header for Raspberry Pi GPIO&lt;br/&gt;
 &amp;nbsp; for use with flat ribbon cables</description>
</package>
<package name="RASPI_BOARD_EDGES_2DRILL_PAD">
<description>Raspberry Pi board, outline is only marked by its edges&lt;br&gt;
including 2 mounting pads for Model B Revision 2.0</description>
</package>
<package name="RASPI_BOARD_EDGES_1DRILL_PAD">
<description>Raspberry Pi board, outline is only marked by its edges&lt;br&gt;
including 1 mounting pad for Model B Revision 2.0</description>
</package>
<package name="RASPI_BOARD_FULL_PAD">
<description>Raspberry Pi board, full outline with position of big connectors + components&lt;br&gt;
including mounting pads for Model B Revision 2.0</description>
</package>
<package name="RASPI_BOARD_THIN_PAD">
<description>Raspberry Pi board
 - 
Thin version with only the width of the GPIO connector and 1 mounting pad</description>
</package>
<package name="RASPI_BOARD_THIN_BOT">
<description>Raspberry Pi board - Thin version with only the width of the GPIO connector and 1 drill hole&lt;p/&gt;
Pads are in "Offset" shape to make them easy to solder from the bottom side&lt;br/&gt;
for single-side PCBs</description>
</package>
<package name="RASPI_BOARD_EDGES_0DRILL">
<description>Raspberry Pi board, outline is only marked by its edges&lt;br&gt;
without any drill holes</description>
</package>
<package name="RASPI_BOARD_THIN">
<description>Raspberry Pi board
 - 
Thin version with only the width of the GPIO connector</description>
</package>
</packages>
<symbols>
<symbol name="RASPI_GPIO">
<description>Generic schematic symbol for the Raspberry Pi GPIO connector</description>
<pin name="5V0" direction="pwr"/>
<pin name="3V3" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="GPIO0"/>
<pin name="GPIO1"/>
<pin name="GPIO2"/>
<pin name="GPIO3"/>
<pin name="GPIO4"/>
<pin name="GPIO5"/>
<pin name="GPIO6"/>
<pin name="GPIO7"/>
<pin name="TXD"/>
<pin name="RXD"/>
<pin name="SPI_MOSI"/>
<pin name="SPI_MISO"/>
<pin name="SPI_SCLK"/>
<pin name="SPI_CE0"/>
<pin name="SPI_CE1"/>
<pin name="N.C.0" direction="nc"/>
<pin name="N.C.1" direction="nc"/>
<pin name="N.C.2" direction="nc"/>
<pin name="N.C.3" direction="nc"/>
<pin name="N.C.4" direction="nc"/>
<pin name="N.C.5" direction="nc"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="RASPI_GPIO" prefix="X">
<description>Only the 2x13 header connector, nothing else</description>
<gates>
<gate name="G$1" symbol="RASPI_GPIO"/>
</gates>
<devices>
<device name="_PIN" package="RASPI_GPIO_PIN">
<connects>
<connect gate="G$1" pin="3V3" pad="1"/>
<connect gate="G$1" pin="5V0" pad="2"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GPIO0" pad="11"/>
<connect gate="G$1" pin="GPIO1" pad="12"/>
<connect gate="G$1" pin="GPIO2" pad="13"/>
<connect gate="G$1" pin="GPIO3" pad="15"/>
<connect gate="G$1" pin="GPIO4" pad="16"/>
<connect gate="G$1" pin="GPIO5" pad="18"/>
<connect gate="G$1" pin="GPIO6" pad="22"/>
<connect gate="G$1" pin="GPIO7" pad="7"/>
<connect gate="G$1" pin="N.C.0" pad="4"/>
<connect gate="G$1" pin="N.C.1" pad="9"/>
<connect gate="G$1" pin="N.C.2" pad="14"/>
<connect gate="G$1" pin="N.C.3" pad="17"/>
<connect gate="G$1" pin="N.C.4" pad="20"/>
<connect gate="G$1" pin="N.C.5" pad="25"/>
<connect gate="G$1" pin="RXD" pad="10"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="SPI_CE0" pad="24"/>
<connect gate="G$1" pin="SPI_CE1" pad="26"/>
<connect gate="G$1" pin="SPI_MISO" pad="21"/>
<connect gate="G$1" pin="SPI_MOSI" pad="19"/>
<connect gate="G$1" pin="SPI_SCLK" pad="23"/>
<connect gate="G$1" pin="TXD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_BOX" package="RASPI_GPIO_BOX">
<connects>
<connect gate="G$1" pin="3V3" pad="1"/>
<connect gate="G$1" pin="5V0" pad="2"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GPIO0" pad="11"/>
<connect gate="G$1" pin="GPIO1" pad="12"/>
<connect gate="G$1" pin="GPIO2" pad="13"/>
<connect gate="G$1" pin="GPIO3" pad="15"/>
<connect gate="G$1" pin="GPIO4" pad="16"/>
<connect gate="G$1" pin="GPIO5" pad="18"/>
<connect gate="G$1" pin="GPIO6" pad="22"/>
<connect gate="G$1" pin="GPIO7" pad="7"/>
<connect gate="G$1" pin="N.C.0" pad="4"/>
<connect gate="G$1" pin="N.C.1" pad="9"/>
<connect gate="G$1" pin="N.C.2" pad="14"/>
<connect gate="G$1" pin="N.C.3" pad="17"/>
<connect gate="G$1" pin="N.C.4" pad="20"/>
<connect gate="G$1" pin="N.C.5" pad="25"/>
<connect gate="G$1" pin="RXD" pad="10"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="SPI_CE0" pad="24"/>
<connect gate="G$1" pin="SPI_CE1" pad="26"/>
<connect gate="G$1" pin="SPI_MISO" pad="21"/>
<connect gate="G$1" pin="SPI_MOSI" pad="19"/>
<connect gate="G$1" pin="SPI_SCLK" pad="23"/>
<connect gate="G$1" pin="TXD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RASPI_BOARD" prefix="X">
<description>Raspberry Pi GPIO connector with markings for the outer dimensions of the Raspberry Pi board&lt;br&gt;
+ drilling holes for the Model B Revision 2.0 board</description>
<gates>
<gate name="G$1" symbol="RASPI_GPIO"/>
</gates>
<devices>
<device name="_E2" package="RASPI_BOARD_EDGES_2DRILL">
<connects>
<connect gate="G$1" pin="3V3" pad="1"/>
<connect gate="G$1" pin="5V0" pad="2"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GPIO0" pad="11"/>
<connect gate="G$1" pin="GPIO1" pad="12"/>
<connect gate="G$1" pin="GPIO2" pad="13"/>
<connect gate="G$1" pin="GPIO3" pad="15"/>
<connect gate="G$1" pin="GPIO4" pad="16"/>
<connect gate="G$1" pin="GPIO5" pad="18"/>
<connect gate="G$1" pin="GPIO6" pad="22"/>
<connect gate="G$1" pin="GPIO7" pad="7"/>
<connect gate="G$1" pin="N.C.0" pad="4"/>
<connect gate="G$1" pin="N.C.1" pad="9"/>
<connect gate="G$1" pin="N.C.2" pad="14"/>
<connect gate="G$1" pin="N.C.3" pad="17"/>
<connect gate="G$1" pin="N.C.4" pad="20"/>
<connect gate="G$1" pin="N.C.5" pad="25"/>
<connect gate="G$1" pin="RXD" pad="10"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="SPI_CE0" pad="24"/>
<connect gate="G$1" pin="SPI_CE1" pad="26"/>
<connect gate="G$1" pin="SPI_MISO" pad="21"/>
<connect gate="G$1" pin="SPI_MOSI" pad="19"/>
<connect gate="G$1" pin="SPI_SCLK" pad="23"/>
<connect gate="G$1" pin="TXD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_F" package="RASPI_BOARD_FULL">
<connects>
<connect gate="G$1" pin="3V3" pad="1"/>
<connect gate="G$1" pin="5V0" pad="2"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GPIO0" pad="11"/>
<connect gate="G$1" pin="GPIO1" pad="12"/>
<connect gate="G$1" pin="GPIO2" pad="13"/>
<connect gate="G$1" pin="GPIO3" pad="15"/>
<connect gate="G$1" pin="GPIO4" pad="16"/>
<connect gate="G$1" pin="GPIO5" pad="18"/>
<connect gate="G$1" pin="GPIO6" pad="22"/>
<connect gate="G$1" pin="GPIO7" pad="7"/>
<connect gate="G$1" pin="N.C.0" pad="4"/>
<connect gate="G$1" pin="N.C.1" pad="9"/>
<connect gate="G$1" pin="N.C.2" pad="14"/>
<connect gate="G$1" pin="N.C.3" pad="17"/>
<connect gate="G$1" pin="N.C.4" pad="20"/>
<connect gate="G$1" pin="N.C.5" pad="25"/>
<connect gate="G$1" pin="RXD" pad="10"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="SPI_CE0" pad="24"/>
<connect gate="G$1" pin="SPI_CE1" pad="26"/>
<connect gate="G$1" pin="SPI_MISO" pad="21"/>
<connect gate="G$1" pin="SPI_MOSI" pad="19"/>
<connect gate="G$1" pin="SPI_SCLK" pad="23"/>
<connect gate="G$1" pin="TXD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_E1" package="RASPI_BOARD_EDGES_1DRILL">
<connects>
<connect gate="G$1" pin="3V3" pad="1"/>
<connect gate="G$1" pin="5V0" pad="2"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GPIO0" pad="11"/>
<connect gate="G$1" pin="GPIO1" pad="12"/>
<connect gate="G$1" pin="GPIO2" pad="13"/>
<connect gate="G$1" pin="GPIO3" pad="15"/>
<connect gate="G$1" pin="GPIO4" pad="16"/>
<connect gate="G$1" pin="GPIO5" pad="18"/>
<connect gate="G$1" pin="GPIO6" pad="22"/>
<connect gate="G$1" pin="GPIO7" pad="7"/>
<connect gate="G$1" pin="N.C.0" pad="4"/>
<connect gate="G$1" pin="N.C.1" pad="9"/>
<connect gate="G$1" pin="N.C.2" pad="14"/>
<connect gate="G$1" pin="N.C.3" pad="17"/>
<connect gate="G$1" pin="N.C.4" pad="20"/>
<connect gate="G$1" pin="N.C.5" pad="25"/>
<connect gate="G$1" pin="RXD" pad="10"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="SPI_CE0" pad="24"/>
<connect gate="G$1" pin="SPI_CE1" pad="26"/>
<connect gate="G$1" pin="SPI_MISO" pad="21"/>
<connect gate="G$1" pin="SPI_MOSI" pad="19"/>
<connect gate="G$1" pin="SPI_SCLK" pad="23"/>
<connect gate="G$1" pin="TXD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_TD" package="RASPI_BOARD_THIN_DRILL">
<connects>
<connect gate="G$1" pin="3V3" pad="1"/>
<connect gate="G$1" pin="5V0" pad="2"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GPIO0" pad="11"/>
<connect gate="G$1" pin="GPIO1" pad="12"/>
<connect gate="G$1" pin="GPIO2" pad="13"/>
<connect gate="G$1" pin="GPIO3" pad="15"/>
<connect gate="G$1" pin="GPIO4" pad="16"/>
<connect gate="G$1" pin="GPIO5" pad="18"/>
<connect gate="G$1" pin="GPIO6" pad="22"/>
<connect gate="G$1" pin="GPIO7" pad="7"/>
<connect gate="G$1" pin="N.C.0" pad="4"/>
<connect gate="G$1" pin="N.C.1" pad="9"/>
<connect gate="G$1" pin="N.C.2" pad="14"/>
<connect gate="G$1" pin="N.C.3" pad="17"/>
<connect gate="G$1" pin="N.C.4" pad="20"/>
<connect gate="G$1" pin="N.C.5" pad="25"/>
<connect gate="G$1" pin="RXD" pad="10"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="SPI_CE0" pad="24"/>
<connect gate="G$1" pin="SPI_CE1" pad="26"/>
<connect gate="G$1" pin="SPI_MISO" pad="21"/>
<connect gate="G$1" pin="SPI_MOSI" pad="19"/>
<connect gate="G$1" pin="SPI_SCLK" pad="23"/>
<connect gate="G$1" pin="TXD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_E1P" package="RASPI_BOARD_EDGES_1DRILL_PAD">
<connects>
<connect gate="G$1" pin="3V3" pad="1"/>
<connect gate="G$1" pin="5V0" pad="2"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GPIO0" pad="11"/>
<connect gate="G$1" pin="GPIO1" pad="12"/>
<connect gate="G$1" pin="GPIO2" pad="13"/>
<connect gate="G$1" pin="GPIO3" pad="15"/>
<connect gate="G$1" pin="GPIO4" pad="16"/>
<connect gate="G$1" pin="GPIO5" pad="18"/>
<connect gate="G$1" pin="GPIO6" pad="22"/>
<connect gate="G$1" pin="GPIO7" pad="7"/>
<connect gate="G$1" pin="N.C.0" pad="4"/>
<connect gate="G$1" pin="N.C.1" pad="9"/>
<connect gate="G$1" pin="N.C.2" pad="14"/>
<connect gate="G$1" pin="N.C.3" pad="17"/>
<connect gate="G$1" pin="N.C.4" pad="20"/>
<connect gate="G$1" pin="N.C.5" pad="25"/>
<connect gate="G$1" pin="RXD" pad="10"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="SPI_CE0" pad="24"/>
<connect gate="G$1" pin="SPI_CE1" pad="26"/>
<connect gate="G$1" pin="SPI_MISO" pad="21"/>
<connect gate="G$1" pin="SPI_MOSI" pad="19"/>
<connect gate="G$1" pin="SPI_SCLK" pad="23"/>
<connect gate="G$1" pin="TXD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_E2P" package="RASPI_BOARD_EDGES_2DRILL_PAD">
<connects>
<connect gate="G$1" pin="3V3" pad="1"/>
<connect gate="G$1" pin="5V0" pad="2"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GPIO0" pad="11"/>
<connect gate="G$1" pin="GPIO1" pad="12"/>
<connect gate="G$1" pin="GPIO2" pad="13"/>
<connect gate="G$1" pin="GPIO3" pad="15"/>
<connect gate="G$1" pin="GPIO4" pad="16"/>
<connect gate="G$1" pin="GPIO5" pad="18"/>
<connect gate="G$1" pin="GPIO6" pad="22"/>
<connect gate="G$1" pin="GPIO7" pad="7"/>
<connect gate="G$1" pin="N.C.0" pad="4"/>
<connect gate="G$1" pin="N.C.1" pad="9"/>
<connect gate="G$1" pin="N.C.2" pad="14"/>
<connect gate="G$1" pin="N.C.3" pad="17"/>
<connect gate="G$1" pin="N.C.4" pad="20"/>
<connect gate="G$1" pin="N.C.5" pad="25"/>
<connect gate="G$1" pin="RXD" pad="10"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="SPI_CE0" pad="24"/>
<connect gate="G$1" pin="SPI_CE1" pad="26"/>
<connect gate="G$1" pin="SPI_MISO" pad="21"/>
<connect gate="G$1" pin="SPI_MOSI" pad="19"/>
<connect gate="G$1" pin="SPI_SCLK" pad="23"/>
<connect gate="G$1" pin="TXD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_FP" package="RASPI_BOARD_FULL_PAD">
<connects>
<connect gate="G$1" pin="3V3" pad="1"/>
<connect gate="G$1" pin="5V0" pad="2"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GPIO0" pad="11"/>
<connect gate="G$1" pin="GPIO1" pad="12"/>
<connect gate="G$1" pin="GPIO2" pad="13"/>
<connect gate="G$1" pin="GPIO3" pad="15"/>
<connect gate="G$1" pin="GPIO4" pad="16"/>
<connect gate="G$1" pin="GPIO5" pad="18"/>
<connect gate="G$1" pin="GPIO6" pad="22"/>
<connect gate="G$1" pin="GPIO7" pad="7"/>
<connect gate="G$1" pin="N.C.0" pad="4"/>
<connect gate="G$1" pin="N.C.1" pad="9"/>
<connect gate="G$1" pin="N.C.2" pad="14"/>
<connect gate="G$1" pin="N.C.3" pad="17"/>
<connect gate="G$1" pin="N.C.4" pad="20"/>
<connect gate="G$1" pin="N.C.5" pad="25"/>
<connect gate="G$1" pin="RXD" pad="10"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="SPI_CE0" pad="24"/>
<connect gate="G$1" pin="SPI_CE1" pad="26"/>
<connect gate="G$1" pin="SPI_MISO" pad="21"/>
<connect gate="G$1" pin="SPI_MOSI" pad="19"/>
<connect gate="G$1" pin="SPI_SCLK" pad="23"/>
<connect gate="G$1" pin="TXD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_TP" package="RASPI_BOARD_THIN_PAD">
<connects>
<connect gate="G$1" pin="3V3" pad="1"/>
<connect gate="G$1" pin="5V0" pad="2"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GPIO0" pad="11"/>
<connect gate="G$1" pin="GPIO1" pad="12"/>
<connect gate="G$1" pin="GPIO2" pad="13"/>
<connect gate="G$1" pin="GPIO3" pad="15"/>
<connect gate="G$1" pin="GPIO4" pad="16"/>
<connect gate="G$1" pin="GPIO5" pad="18"/>
<connect gate="G$1" pin="GPIO6" pad="22"/>
<connect gate="G$1" pin="GPIO7" pad="7"/>
<connect gate="G$1" pin="N.C.0" pad="4"/>
<connect gate="G$1" pin="N.C.1" pad="9"/>
<connect gate="G$1" pin="N.C.2" pad="14"/>
<connect gate="G$1" pin="N.C.3" pad="17"/>
<connect gate="G$1" pin="N.C.4" pad="20"/>
<connect gate="G$1" pin="N.C.5" pad="25"/>
<connect gate="G$1" pin="RXD" pad="10"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="SPI_CE0" pad="24"/>
<connect gate="G$1" pin="SPI_CE1" pad="26"/>
<connect gate="G$1" pin="SPI_MISO" pad="21"/>
<connect gate="G$1" pin="SPI_MOSI" pad="19"/>
<connect gate="G$1" pin="SPI_SCLK" pad="23"/>
<connect gate="G$1" pin="TXD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_TB" package="RASPI_BOARD_THIN_BOT">
<connects>
<connect gate="G$1" pin="3V3" pad="1"/>
<connect gate="G$1" pin="5V0" pad="2"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GPIO0" pad="11"/>
<connect gate="G$1" pin="GPIO1" pad="12"/>
<connect gate="G$1" pin="GPIO2" pad="13"/>
<connect gate="G$1" pin="GPIO3" pad="15"/>
<connect gate="G$1" pin="GPIO4" pad="16"/>
<connect gate="G$1" pin="GPIO5" pad="18"/>
<connect gate="G$1" pin="GPIO6" pad="22"/>
<connect gate="G$1" pin="GPIO7" pad="7"/>
<connect gate="G$1" pin="N.C.0" pad="4"/>
<connect gate="G$1" pin="N.C.1" pad="9"/>
<connect gate="G$1" pin="N.C.2" pad="14"/>
<connect gate="G$1" pin="N.C.3" pad="17"/>
<connect gate="G$1" pin="N.C.4" pad="20"/>
<connect gate="G$1" pin="N.C.5" pad="25"/>
<connect gate="G$1" pin="RXD" pad="10"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="SPI_CE0" pad="24"/>
<connect gate="G$1" pin="SPI_CE1" pad="26"/>
<connect gate="G$1" pin="SPI_MISO" pad="21"/>
<connect gate="G$1" pin="SPI_MOSI" pad="19"/>
<connect gate="G$1" pin="SPI_SCLK" pad="23"/>
<connect gate="G$1" pin="TXD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_E0" package="RASPI_BOARD_EDGES_0DRILL">
<connects>
<connect gate="G$1" pin="3V3" pad="1"/>
<connect gate="G$1" pin="5V0" pad="2"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GPIO0" pad="11"/>
<connect gate="G$1" pin="GPIO1" pad="12"/>
<connect gate="G$1" pin="GPIO2" pad="13"/>
<connect gate="G$1" pin="GPIO3" pad="15"/>
<connect gate="G$1" pin="GPIO4" pad="16"/>
<connect gate="G$1" pin="GPIO5" pad="18"/>
<connect gate="G$1" pin="GPIO6" pad="22"/>
<connect gate="G$1" pin="GPIO7" pad="7"/>
<connect gate="G$1" pin="N.C.0" pad="4"/>
<connect gate="G$1" pin="N.C.1" pad="9"/>
<connect gate="G$1" pin="N.C.2" pad="14"/>
<connect gate="G$1" pin="N.C.3" pad="17"/>
<connect gate="G$1" pin="N.C.4" pad="20"/>
<connect gate="G$1" pin="N.C.5" pad="25"/>
<connect gate="G$1" pin="RXD" pad="10"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="SPI_CE0" pad="24"/>
<connect gate="G$1" pin="SPI_CE1" pad="26"/>
<connect gate="G$1" pin="SPI_MISO" pad="21"/>
<connect gate="G$1" pin="SPI_MOSI" pad="19"/>
<connect gate="G$1" pin="SPI_SCLK" pad="23"/>
<connect gate="G$1" pin="TXD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_T" package="RASPI_BOARD_THIN">
<connects>
<connect gate="G$1" pin="3V3" pad="1"/>
<connect gate="G$1" pin="5V0" pad="2"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GPIO0" pad="11"/>
<connect gate="G$1" pin="GPIO1" pad="12"/>
<connect gate="G$1" pin="GPIO2" pad="13"/>
<connect gate="G$1" pin="GPIO3" pad="15"/>
<connect gate="G$1" pin="GPIO4" pad="16"/>
<connect gate="G$1" pin="GPIO5" pad="18"/>
<connect gate="G$1" pin="GPIO6" pad="22"/>
<connect gate="G$1" pin="GPIO7" pad="7"/>
<connect gate="G$1" pin="N.C.0" pad="4"/>
<connect gate="G$1" pin="N.C.1" pad="9"/>
<connect gate="G$1" pin="N.C.2" pad="14"/>
<connect gate="G$1" pin="N.C.3" pad="17"/>
<connect gate="G$1" pin="N.C.4" pad="20"/>
<connect gate="G$1" pin="N.C.5" pad="25"/>
<connect gate="G$1" pin="RXD" pad="10"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="SPI_CE0" pad="24"/>
<connect gate="G$1" pin="SPI_CE1" pad="26"/>
<connect gate="G$1" pin="SPI_MISO" pad="21"/>
<connect gate="G$1" pin="SPI_MOSI" pad="19"/>
<connect gate="G$1" pin="SPI_SCLK" pad="23"/>
<connect gate="G$1" pin="TXD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
