Summary: Constants | Inherited Constants | Methods | Inherited Methods | [Expand All]
public final class

# WearableStatusCodes

extends CommonStatusCodes

java.lang.Object
↳ | com.google.android.gms.common.api.CommonStatusCodes
| ↳ | com.google.android.gms.wearable.WearableStatusCodes

## Class Overview

Error codes for wearable API failures. These values may be returned by APIs to indicate the success or failure of a request.

## Summary

Constants
int | ASSET_UNAVAILABLE | Indicates that the requested asset is unavailable.
int | DATA_ITEM_TOO_LARGE | Indicates that the data item was too large to set.
int | DUPLICATE_CAPABILITY | Indicates that the specified capability already exists.
int | DUPLICATE_LISTENER | Indicates that the specified listener is already registered.
int | INVALID_TARGET_NODE | Indicates that the targeted node is not a valid node in the wearable network.
int | TARGET_NODE_NOT_CONNECTED | Indicates that the targeted node is not accessible in the wearable network.
int | UNKNOWN_CAPABILITY | Indicates that the specified capability is not recognized.
int | UNKNOWN_LISTENER | Indicates that the specified listener is not recognized.
int | WIFI_CREDENTIAL_SYNC_NO_CREDENTIAL_FETCHED | Indicates that the WiFi credential sync no credential fetched.

[Expand] Inherited Constants
From class com.google.android.gms.common.api.CommonStatusCodes
int | API_NOT_CONNECTED | The client attempted to call a method from an API that failed to connect.
int | CANCELED | The result was canceled either due to client disconnect or `cancel()`.
int | DEVELOPER_ERROR | The application is misconfigured.
int | ERROR | The operation failed with no more detailed information.
int | INTERNAL_ERROR | An internal error occurred.
int | INTERRUPTED | A blocking call was interrupted while waiting and did not run to completion.
int | INVALID_ACCOUNT | The client attempted to connect to the service with an invalid account name specified.
int | NETWORK_ERROR | A network error occurred.
int | RESOLUTION_REQUIRED | Completing the operation requires some form of resolution.
int | SERVICE_DISABLED | This constant is deprecated. This case handled during connection, not during API requests. No results should be returned with this status code.
int | SERVICE_VERSION_UPDATE_REQUIRED | This constant is deprecated. This case handled during connection, not during API requests. No results should be returned with this status code.
int | SIGN_IN_REQUIRED | The client attempted to connect to the service but the user is not signed in.
int | SUCCESS | The operation was successful.
int | SUCCESS_CACHE | The operation was successful, but was used the device's cache.
int | TIMEOUT | Timed out while awaiting the result.

Public Methods
static String | getStatusCodeString(int statusCode) Returns an untranslated debug (not user-friendly!) string based on the current status code.

[Expand] Inherited Methods
From class com.google.android.gms.common.api.CommonStatusCodes
static String | getStatusCodeString(int statusCode)
From class java.lang.Object
Object | clone()
boolean | equals(Object arg0)
void | finalize()
final Class<?> | getClass()
int | hashCode()
final void | notify()
final void | notifyAll()
String | toString()
final void | wait(long arg0, int arg1)
final void | wait(long arg0)
final void | wait()

## Constants

#### public static final int ASSET_UNAVAILABLE

Indicates that the requested asset is unavailable.

Constant Value: 4005 (0x00000fa5)

#### public static final int DATA_ITEM_TOO_LARGE

Indicates that the data item was too large to set.

Constant Value: 4003 (0x00000fa3)

#### public static final int DUPLICATE_CAPABILITY

Indicates that the specified capability already exists.

Constant Value: 4006 (0x00000fa6)

#### public static final int DUPLICATE_LISTENER

Indicates that the specified listener is already registered.

Constant Value: 4001 (0x00000fa1)

#### public static final int INVALID_TARGET_NODE

Indicates that the targeted node is not a valid node in the wearable network.

Constant Value: 4004 (0x00000fa4)

#### public static final int TARGET_NODE_NOT_CONNECTED

Indicates that the targeted node is not accessible in the wearable network.

Constant Value: 4000 (0x00000fa0)

#### public static final int UNKNOWN_CAPABILITY

Indicates that the specified capability is not recognized.

Constant Value: 4007 (0x00000fa7)

#### public static final int UNKNOWN_LISTENER

Indicates that the specified listener is not recognized.

Constant Value: 4002 (0x00000fa2)

#### public static final int WIFI_CREDENTIAL_SYNC_NO_CREDENTIAL_FETCHED

Indicates that the WiFi credential sync no credential fetched.

Constant Value: 4008 (0x00000fa8)

## Public Methods

#### public static String getStatusCodeString (int statusCode)

Returns an untranslated debug (not user-friendly!) string based on the current status code.