analysis(xf fields center) ""
analysis(xf fields dec) ""
analysis(xf fields designVar) ""
analysis(xf fields dev) "/Vvin"
analysis(xf fields deviceParam) "dc"
analysis(xf fields enable) (t)
analysis(xf fields freq) "1"
analysis(xf fields incrType) "Automatic"
analysis(xf fields lin) ""
analysis(xf fields log) ""
analysis(xf fields mod) ""
analysis(xf fields modelParam) ""
analysis(xf fields n) ""
analysis(xf fields outType) "voltage"
analysis(xf fields p) "Vout"
analysis(xf fields param) "dc"
analysis(xf fields probe) ""
analysis(xf fields rangeType) "Start-Stop"
analysis(xf fields span) ""
analysis(xf fields start) "0"
analysis(xf fields step) ""
analysis(xf fields stepTypeLin) "Step Size"
analysis(xf fields stepTypeLog) "Points Per Decade"
analysis(xf fields stop) "1"
analysis(xf fields sweep) "Component Parameter"
analysis(xf fields sweepChange) nil
analysis(xf fields useDiscrete) nil
analysis(xf fields values) nil
analysis(xf options additionalParams) ""
analysis(xf options annotate) "status"
analysis(xf options force) ""
analysis(xf options nestlvl) ""
analysis(xf options oppoint) ""
analysis(xf options prevoppoint) ""
analysis(xf options readforce) ""
analysis(xf options readns) ""
analysis(xf options restart) ""
analysis(xf options save) ""
analysis(xf options stimuli) ""
