
**** 07/17/05 11:47:33 ********* PSpice 9.2 (Mar 2000) ******** ID# 1 ********

 ** Profile: "SCHEMATIC1-simu01"  [ D:\WORKAREA\PSPICE\pass gate\porte-SCHEMATIC1-simu01.sim ] 


 ****     CIRCUIT DESCRIPTION


******************************************************************************




** Creating circuit file "porte-SCHEMATIC1-simu01.sim.cir" 
** WARNING: THIS AUTOMATICALLY GENERATED FILE MAY BE OVERWRITTEN BY SUBSEQUENT SIMULATIONS

*Libraries: 
* Local Libraries :
* From [PSPICE NETLIST] section of D:\Orcad\PSpice\PSpice.ini file:
.lib "nom.lib" 

*Analysis directives: 
.TRAN  0 20us 0 
.PROBE V(*) I(*) W(*) D(*) NOISE(*) 
.INC ".\porte-SCHEMATIC1.net" 



**** INCLUDING porte-SCHEMATIC1.net ****
* source PORTE
U_DSTM1         STIM(1,1) $G_DPWR $G_DGND IN IO_STM IO_LEVEL=0 
+ 0 0
+ +5uS 1
+REPEAT FOREVER
+ +5uS 0
+  +5uS 1
+ ENDREPEAT
X_U6A         Q2 Q0 $G_DPWR $G_DGND 7404 PARAMS:
+ IO_LEVEL=0 MNTYMXDLY=0
X_U7A         N02208 N02245 $G_DPWR $G_DGND 7404 PARAMS:
+ IO_LEVEL=0 MNTYMXDLY=0
X_U2A         IN Q3 N02423 $G_DPWR $G_DGND 7402 PARAMS:
+ IO_LEVEL=0 MNTYMXDLY=0
V_V1         VDD 0  DC 2.5V
X_U8A         N02245 Q3 $G_DPWR $G_DGND 7404 PARAMS:
+ IO_LEVEL=0 MNTYMXDLY=0
V_V2         VSS 0  DC -2.5V
X_U9A         Q3 Q1 $G_DPWR $G_DGND 7404 PARAMS:
+ IO_LEVEL=0 MNTYMXDLY=0
X_U3A         Q2 N02168 N02208 $G_DPWR $G_DGND 7402 PARAMS:
+ IO_LEVEL=0 MNTYMXDLY=0
X_U10A         IN N02168 $G_DPWR $G_DGND 7404 PARAMS:
+ IO_LEVEL=0 MNTYMXDLY=0
X_U1A         IN OUT $G_DPWR $G_DGND 7404 PARAMS:
+ IO_LEVEL=0 MNTYMXDLY=0
X_U4A         N02423 N02460 $G_DPWR $G_DGND 7404 PARAMS:
+ IO_LEVEL=0 MNTYMXDLY=0
X_U5A         N02460 Q2 $G_DPWR $G_DGND 7404 PARAMS:
+ IO_LEVEL=0 MNTYMXDLY=0

**** RESUMING porte-SCHEMATIC1-simu01.sim.cir ****
.END

**** 07/17/05 11:47:33 ********* PSpice 9.2 (Mar 2000) ******** ID# 1 ********

 ** Profile: "SCHEMATIC1-simu01"  [ D:\WORKAREA\PSPICE\pass gate\porte-SCHEMATIC1-simu01.sim ] 


 ****     Digital Gate MODEL PARAMETERS


******************************************************************************




               D_04            D_02            
      TPLHMN    4.800000E-09    4.800000E-09 
      TPLHTY   12.000000E-09   12.000000E-09 
      TPLHMX   22.000000E-09   22.000000E-09 
      TPHLMN    3.200000E-09    3.200000E-09 
      TPHLTY    8.000000E-09    8.000000E-09 
      TPHLMX   15.000000E-09   15.000000E-09 


**** 07/17/05 11:47:33 ********* PSpice 9.2 (Mar 2000) ******** ID# 1 ********

 ** Profile: "SCHEMATIC1-simu01"  [ D:\WORKAREA\PSPICE\pass gate\porte-SCHEMATIC1-simu01.sim ] 


 ****     Digital IO  MODEL PARAMETERS


******************************************************************************




               IO_STM          IO_STD          
        DRVL    0             104            
        DRVH    0              96.4          
       AtoD1                 AtoD_STD        
       AtoD2                 AtoD_STD_NX     
       AtoD3                 AtoD_STD        
       AtoD4                 AtoD_STD_NX     
       DtoA1 DtoA_STM        DtoA_STD        
       DtoA2 DtoA_STM        DtoA_STD        
       DtoA3 DtoA_STM        DtoA_STD        
       DtoA4 DtoA_STM        DtoA_STD        
      TSWHL1                    1.511000E-09 
      TSWHL2                    1.487000E-09 
      TSWHL3                    1.511000E-09 
      TSWHL4                    1.487000E-09 
      TSWLH1                    3.517000E-09 
      TSWLH2                    3.564000E-09 
      TSWLH3                    3.517000E-09 
      TSWLH4                    3.564000E-09 
       TPWRT  100.000000E+03  100.000000E+03 


**** 07/17/05 11:47:33 ********* PSpice 9.2 (Mar 2000) ******** ID# 1 ********

 ** Profile: "SCHEMATIC1-simu01"  [ D:\WORKAREA\PSPICE\pass gate\porte-SCHEMATIC1-simu01.sim ] 


 ****     INITIAL TRANSIENT SOLUTION       TEMPERATURE =   27.000 DEG C


******************************************************************************



 NODE   VOLTAGE     NODE   VOLTAGE     NODE   VOLTAGE     NODE   VOLTAGE


(  VDD)    2.5000  (  VSS)   -2.5000  



 DGTL NODE : STATE  DGTL NODE : STATE  DGTL NODE : STATE  DGTL NODE : STATE


(      Q1) : 1     (  N02460) : 0     (  N02245) : 1     (     OUT) : 1         

(      Q2) : 1     (      IN) : 0     (  N02168) : 1     (  N02423) : 1         

(  N02208) : 0     (      Q3) : 0     (      Q0) : 0     




    VOLTAGE SOURCE CURRENTS
    NAME         CURRENT

    V_V1         0.000E+00
    V_V2         0.000E+00

    TOTAL POWER DISSIPATION   0.00E+00  WATTS



          JOB CONCLUDED

          TOTAL JOB TIME             .05
