@OrCAD Simulation Server Version: 1.0

@Settings: 0 1
@General:
ProfileName= "TRAN" 
ProfileFile= "dual_slope-DUAL_SLOPE-TRAN.sim" 
DesignFile= "dual_slope.dsn" 0 
ProjectFile= "dual_slope.opj" 
NetlistFile= "" 
RootSchematics= "DUAL_SLOPE" 
DataFile= "dual_slope-DUAL_SLOPE-TRAN.dat" 
OutFile= "dual_slope-DUAL_SLOPE-TRAN.out" 
Notes=
@#$BEGINNOTES
Translated design from D:\WORKAREA\PSPICE\pass gate\dual_slope.sch on Sunday, July 17, 2005 17:41:42
@#$ENDNOTES
@End General
@Analysis: 0 1
+0 0 0 
+0 "100ms" 
+1 "10u" 
+2 "" 
+3 "" 
+4 "" 
+5 "" 
+6 "" 
@End Analysis
@Analysis: 1 0
+0 0 0
+0 "101" 
+1 "10" 
+2 "1.00K" 
+3 "" 
+4 "" 
+5 "" 
@End Analysis
@Analysis: 2 0
+0 0
+0 "" 
+1 "" 
+2 "" 
+3 "" 
+4 "" 
+5 "" 
+6 "" 
+7 "" 
@End Analysis
@Analysis: 3 1
+1 0 0
+0 "" 
+1 "" 
+2 "" 
@End Analysis
@Analysis: 4 0
+0 1 0 0 0 0 0 0 
+0 "" 
+1 "" 
+2 "" 
+3 "" 
+4 "" 
+5 "" 
+6 "" 
+7 "" 
@End Analysis
@Analysis: 5 0
+1 4
+0 "" 
+1 "" 
+2 "" 
+3 "" 
+4 "" 
+5 "" 
+6 "" 
+7 "" 
@End Analysis
@Analysis: 6 0
+1 
+0 "27" 
@End Analysis
@Analysis: 7 0
+1 0
+0 "" 
+1 "" 
+2 "" 
+3 "" 
+4 "" 
+5 "" 
@End Analysis
@Analysis: 8 0
+0 
+0 "" 
+1 "" 
+2 "" 
+3 "" 
+4 "" 
+5 "" 
@End Analysis
@Analysis: 9 0
+0 "" 
@End Analysis
@Analysis: 10 0
+1 4
+0 "" 
+1 "" 
+2 "" 
+3 "" 
+4 "" 
+5 "" 
+6 "" 
+7 "" 
@End Analysis
@Analysis: 11 1
+ 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 
+ DIGINITSTATE "0"
@End Analysis
@Analysis: 12 1
+0 0
@End Analysis
@Analysis: 13 1
+1 1 1 0
@End Analysis
