
**** 07/15/05 22:17:16 ********* PSpice 9.2 (Mar 2000) ******** ID# 1 ********

 ** Profile: "SCHEMATIC1-Bode"  [ D:\workarea\pspice\RC\bode-SCHEMATIC1-Bode.sim ] 


 ****     CIRCUIT DESCRIPTION


******************************************************************************




** Creating circuit file "bode-SCHEMATIC1-Bode.sim.cir" 
** WARNING: THIS AUTOMATICALLY GENERATED FILE MAY BE OVERWRITTEN BY SUBSEQUENT SIMULATIONS

*Libraries: 
* Local Libraries :
* From [PSPICE NETLIST] section of D:\Orcad\PSpice\PSpice.ini file:
.lib "nom.lib" 

*Analysis directives: 
.AC DEC 20 1Hz 1000000Hz
.PROBE V(*) I(*) W(*) D(*) NOISE(*) 
.INC ".\bode-SCHEMATIC1.net" 



**** INCLUDING bode-SCHEMATIC1.net ****
* source BODE
V_V1         N00015 0 DC 0Vdc AC 1Vac 
C_C1         0 N00009  0.01uF  
R_R1         N00015 N00009  100k  

**** RESUMING bode-SCHEMATIC1-Bode.sim.cir ****
.END

**** 07/15/05 22:17:16 ********* PSpice 9.2 (Mar 2000) ******** ID# 1 ********

 ** Profile: "SCHEMATIC1-Bode"  [ D:\workarea\pspice\RC\bode-SCHEMATIC1-Bode.sim ] 


 ****     SMALL SIGNAL BIAS SOLUTION       TEMPERATURE =   27.000 DEG C


******************************************************************************



 NODE   VOLTAGE     NODE   VOLTAGE     NODE   VOLTAGE     NODE   VOLTAGE


(N00009)    0.0000 (N00015)    0.0000 




    VOLTAGE SOURCE CURRENTS
    NAME         CURRENT

    V_V1         0.000E+00

    TOTAL POWER DISSIPATION   0.00E+00  WATTS



          JOB CONCLUDED

          TOTAL JOB TIME             .02
