
**** 02/01/01 19:43:25 *********** Evaluation PSpice (Nov 1999) **************

 ** Profile: "SCHEMATIC1-one"  [ D:\Bode\lab1b-schematic1-one.sim ] 


 ****     CIRCUIT DESCRIPTION


******************************************************************************




** Creating circuit file "lab1b-schematic1-one.sim.cir" 
** WARNING: THIS AUTOMATICALLY GENERATED FILE MAY BE OVERWRITTEN BY SUBSEQUENT SIMULATIONS

*Libraries: 
* Local Libraries :
* From [PSPICE NETLIST] section of pspiceev.ini file:
.lib "nom.lib" 

*Analysis directives: 
.AC DEC 20 1Hz 1000000Hz
.PROBE 
.INC "lab1b-SCHEMATIC1.net" 


**** INCLUDING lab1b-SCHEMATIC1.net ****
* source LAB1B
V_V1         N00015 0 DC 0Vdc AC 1Vac 
C_C1         0 N00009  0.01uF  
R_R1         N00015 N00009  100k  

**** RESUMING lab1b-schematic1-one.sim.cir ****
.INC "lab1b-SCHEMATIC1.als"



**** INCLUDING lab1b-SCHEMATIC1.als ****
.ALIASES
V_V1            V1(+=N00015 -=0 )
C_C1            C1(1=0 2=N00009 )
R_R1            R1(1=N00015 2=N00009 )
.ENDALIASES

**** RESUMING lab1b-schematic1-one.sim.cir ****
.END

**** 02/01/01 19:43:25 *********** Evaluation PSpice (Nov 1999) **************

 ** Profile: "SCHEMATIC1-one"  [ D:\Bode\lab1b-schematic1-one.sim ] 


 ****     SMALL SIGNAL BIAS SOLUTION       TEMPERATURE =   27.000 DEG C


******************************************************************************



 NODE   VOLTAGE     NODE   VOLTAGE     NODE   VOLTAGE     NODE   VOLTAGE


(N00009)    0.0000 (N00015)    0.0000 




    VOLTAGE SOURCE CURRENTS
    NAME         CURRENT

    V_V1         0.000E+00

    TOTAL POWER DISSIPATION   0.00E+00  WATTS



          JOB CONCLUDED

          TOTAL JOB TIME             .07
