@OrCAD Simulation Server Version: 1.0

@Settings: 1 1
@General:
ProfileName= "Vout(Vin)" 
ProfileFile= "ref-SCHEMATIC1-Vout(Vin).sim" 
DesignFile= "ref.dsn" 0 
ProjectFile= "ref.opj" 
NetlistFile= "" 
RootSchematics= "SCHEMATIC1" 
DataFile= "ref-SCHEMATIC1-Vout(Vin).dat" 
OutFile= "ref-SCHEMATIC1-Vout(Vin).out" 
Notes=
@#$BEGINNOTES
@#$ENDNOTES
@End General
@Analysis: 0 0
+0 0 0 
+0 "1000ns" 
+1 "" 
+2 "0" 
+3 "" 
+4 "" 
+5 "" 
+6 "" 
@End Analysis
@Analysis: 1 0
+2 0
+0 "" 
+1 "" 
+2 "" 
+3 "" 
+4 "" 
+5 "" 
@End Analysis
@Analysis: 2 1
+0 0
+0 "V1" 
+1 "" 
+2 "" 
+3 "" 
+4 "5" 
+5 "12" 
+6 "0.1" 
+7 "" 
@End Analysis
@Analysis: 3 0
+0 0 0
+0 "" 
+1 "" 
+2 "" 
@End Analysis
@Analysis: 4 0
+0 0 0 0 0 0 1 0 
+0 "" 
+1 "" 
+2 "" 
+3 "" 
+4 "" 
+5 "" 
+6 "" 
+7 "" 
@End Analysis
@Analysis: 5 0
+0 0
+0 "" 
+1 "" 
+2 "" 
+3 "" 
+4 "" 
+5 "" 
+6 "" 
+7 "" 
@End Analysis
@Analysis: 6 0
+1 
+0 "" 
@End Analysis
@Analysis: 7 0
+0 0
+0 "" 
+1 "" 
+2 "" 
+3 "" 
+4 "" 
+5 "" 
@End Analysis
@Analysis: 8 0
+0 
+0 "" 
+1 "" 
+2 "" 
+3 "" 
+4 "" 
+5 "" 
@End Analysis
@Analysis: 9 0
+0 "" 
@End Analysis
@Analysis: 10 0
+0 0
+0 "" 
+1 "" 
+2 "" 
+3 "" 
+4 "" 
+5 "" 
+6 "" 
+7 "" 
@End Analysis
@Analysis: 11 1
+ 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 
@End Analysis
@Analysis: 12 0
+2 0
@End Analysis
@Analysis: 13 1
+0 1 0 0
@End Analysis
