#environement:
#EVITER DE SAUVER UN ENVIRONNEMNT !

$WORK_PATH ==/user/ra115c/routeur/SMOS10W/$BLOCKNAME


Conductor Depth 32
Keepout Depth	32
##(nb les  Conductor Depth et Keepout Depth du fichier rules prime sur ceux
###definis dans l'environemet)




Weak Connection 
##(vcr consider that 2 pins are connected inside by a layer with a strong resistivity(POLY)

## Strong connection
##(vcr consider that 2 pins are connected inside by a layer with a weak resistivity(METAL)

Full Connectivity
Interlayer Rules

Rule:
$WORK_PATH/smos10w_digital_block.rules

Export to directory:
$WORK_PATH/$BLOCKNAME


-noclean -path2twire_1 
-do $WORK_PATH/$BLOCKNAME/setup_smos10w.do 
-did $WORK_PATH/$BLOCKNAME/$BLOCKNAME.log
