
                  Here is a quick summary of added bindkeys !!!
                  ---------------------------------------------


                  ******** LSW LAYER VISIBILITY : ********

                     Key ` : Select "poly drawing" layer in LSW
               Keys 1 to X : Select "metalX drawing" level in LSW
              Shift 1 to X : Toggle visibility of all metalX layers and associated vias
                Alt 1 to X : Displays only metalX layers and associated vias
                             ( where X is the last metal level number )

                 Key space : Displays all layers and refresh

                    Alt, p : Displays only pins & label routing layers



                  ******** METALS & VIAS : ********

       Shift, KEYPAD Enter : Change layer purpose of selected shapes (dg, pin ...)

           Shift, KEYPAD - : Swap metal layer or via to previous level
           Shift, KEYPAD + : Swap metal layer or via to next level
            Ctrl, KEYPAD - : Copy selected vias in previous level
            Ctrl, KEYPAD + : Copy selected vias in next level
            Shift KEYPAD 0 : Change contact justification from center-center to lower-left

        Shift, Arrows keys : Increase/Decrease rows/columns contact number 
  Ctrl, Shift, Arrows keys : Increase/Decrease rows/columns contact number on the right/up side



                  ******** LABELS : ********

              Shift, Key [ : Decrease Label size by 25%
              Shift, Key ] : Increase Label size by 25%



                  ******** INSTANCES : ********

                 Shift, F6 : Flip updside-down selected instances
                 Shift, F7 : Flip sideways selected instances
  
                    Alt, o : open selected instance in a new window
             Alt, Shift, C : Copy selected instances in current library and update instances library name



                  ******** When using COPY or MOVE command : ********

                    Key F6 : UpsideDown
                    Key F7 : Sideways



                  ******** PROBE on schematic and layout (with connectivity) : ********

                    Key 9 : highlight net
                    Key 0 : remove all highlight



                  ******** MISC : ********

                      TAB : Center window on mouse point & zoom in
                 Ctrl, e  : In layout window, go to Edit Mode
                       j  : Set snap mode to AnyAngle
