
**** 07/15/05 23:21:49 ********* PSpice 9.2 (Mar 2000) ******** ID# 1 ********

 ** Profile: "SCHEMATIC1-simulations"  [ D:\WORKAREA\PSPICE\Amplificateur\project ii-schematic1-simulations.sim ] 


 ****     CIRCUIT DESCRIPTION


******************************************************************************




** Creating circuit file "project ii-schematic1-simulations.sim.cir" 
** WARNING: THIS AUTOMATICALLY GENERATED FILE MAY BE OVERWRITTEN BY SUBSEQUENT SIMULATIONS

*Libraries: 
* Local Libraries :
.LIB ".\project ii.lib" 
* From [PSPICE NETLIST] section of D:\Orcad\PSpice\PSpice.ini file:
.lib "nom.lib" 

*Analysis directives: 
.TRAN  0 25ms 0 
.PROBE V(*) I(*) W(*) D(*) NOISE(*) 
.INC ".\Project II-SCHEMATIC1.net" 



**** INCLUDING "Project II-SCHEMATIC1.net" ****
* source PROJECT II
R_R13         0 N40792  20k  
R_R16         0 N43298  4.3k  
V_V6         N17712 0  
+SIN 0 0.025m 100 0 0 0
R_R2         0 N17627  4.3k  
R_R17         0 N43235  20k  
R_R3         N17656 N18052  40k  
Q_Q2         N33013 N17656 N17627 Q2N2222
R_R4         0 N17656  20k  
C_C1         N17712 N17656  300mF  
C_C2         N40935 N43235  300mF  
R_R9         0 N44123  6k  
Q_Q1         N40935 N40792 N40855 Q2N2222
R_R10         N40935 N18052  9.1k  
R_R1         N33013 N18052  9.3k  
Q_Q3         N43437 N43235 N43298 Q2N2222
R_R11         N40792 N18052  40k  
R_R14         N43437 N18052  9.3k  
C_C8         N43298 N44123  300mF  
C_C4         0 N40855  300mF  
R_R12         0 N40855  4.3k  
V_V1         N18052 0 15Vdc
R_R15         N43235 N18052  40k  
C_C5         N17627 N40792  300mF  

**** RESUMING "project ii-schematic1-simulations.sim.cir" ****
.END

WARNING -- Library file "D:\WORKAREA\PSPICE\Amplificateur\project ii.lib" has changed since index file "project ii.ind" was created.
WARNING -- The timestamp changed from Fri Apr 27 02:42:26 2001 to Thu Apr 26 16:42:26 2001.
Making new index file "project ii.ind" for library file "project ii.lib"
Index has 1 entries from 1 file(s).

**** 07/15/05 23:21:49 ********* PSpice 9.2 (Mar 2000) ******** ID# 1 ********

 ** Profile: "SCHEMATIC1-simulations"  [ D:\WORKAREA\PSPICE\Amplificateur\project ii-schematic1-simulations.sim ] 


 ****     BJT MODEL PARAMETERS


******************************************************************************




               Q2N2222         
               NPN             
          IS   14.340000E-15 
          BF  100            
          NF    1            
         VAF   74.03         
         IKF     .2847       
         ISE   14.340000E-15 
          NE    1.307        
          BR    6.092        
          NR    1            
          RB   10            
          RC    1            
         CJE   22.010000E-12 
         MJE     .377        
         CJC    7.306000E-12 
         MJC     .3416       
          TF  411.100000E-12 
         XTF    3            
         VTF    1.7          
         ITF     .6          
          TR   46.910000E-09 
         XTB    1.5          
          CN    2.42         
           D     .87         


**** 07/15/05 23:21:49 ********* PSpice 9.2 (Mar 2000) ******** ID# 1 ********

 ** Profile: "SCHEMATIC1-simulations"  [ D:\WORKAREA\PSPICE\Amplificateur\project ii-schematic1-simulations.sim ] 


 ****     INITIAL TRANSIENT SOLUTION       TEMPERATURE =   27.000 DEG C


******************************************************************************



 NODE   VOLTAGE     NODE   VOLTAGE     NODE   VOLTAGE     NODE   VOLTAGE


(N17627)    4.1923 (N17656)    4.8369 (N17712)    0.0000 (N18052)   15.0000     

(N33013)    6.0467 (N40792)    4.8373 (N40855)    4.1927 (N40935)    6.2381     

(N43235)    4.8369 (N43298)    4.1923 (N43437)    6.0467 (N44123)    0.0000 




    VOLTAGE SOURCE CURRENTS
    NAME         CURRENT

    V_V6         0.000E+00
    V_V1        -3.651E-03

    TOTAL POWER DISSIPATION   5.48E-02  WATTS



          JOB CONCLUDED

          TOTAL JOB TIME             .05
