
**** 07/15/05 23:08:00 ********* PSpice 9.2 (Mar 2000) ******** ID# 1 ********

 ** Profile: "SCHEMATIC1-transitoire"  [ D:\workarea\pspice\AOP\integrateur en cascade-SCHEMATIC1-transitoire.sim ] 


 ****     CIRCUIT DESCRIPTION


******************************************************************************




** Creating circuit file "integrateur en cascade-SCHEMATIC1-transitoire.sim.cir" 
** WARNING: THIS AUTOMATICALLY GENERATED FILE MAY BE OVERWRITTEN BY SUBSEQUENT SIMULATIONS

*Libraries: 
* Local Libraries :
* From [PSPICE NETLIST] section of D:\Orcad\PSpice\PSpice.ini file:
.lib "nom.lib" 

*Analysis directives: 
.TRAN  0 2s 0 SKIPBP 
.PROBE V(*) I(*) W(*) D(*) NOISE(*) 
.INC ".\integrateur en cascade-SCHEMATIC1.net" 



**** INCLUDING "integrateur en cascade-SCHEMATIC1.net" ****
* source INTEGRATEUR EN CASCADE
C_C2         N24752 N24652  10n  
C_C1         N22791 N22759  10n  
R_R2         N22753 N22759  10k  
X_U20         0 N22759 N24519 N22837 N22791 LM741
V_V1         N22753 0  
+PULSE 0.5m 0 0 0 0 0.5ms 1ms
V_V3         N24519 0 12Vdc
X_U21         0 N24652 N27621 N24748 N24752 AD741
R_R1         N22791 N24652  10k  
V_V4         0 N22837 12Vdc
V_V6         N27621 0 12Vdc
V_V5         0 N24748 12Vdc

**** RESUMING "integrateur en cascade-SCHEMATIC1-transitoire.sim.cir" ****
.END

**** 07/15/05 23:08:00 ********* PSpice 9.2 (Mar 2000) ******** ID# 1 ********

 ** Profile: "SCHEMATIC1-transitoire"  [ D:\workarea\pspice\AOP\integrateur en cascade-SCHEMATIC1-transitoire.sim ] 


 ****     Diode MODEL PARAMETERS


******************************************************************************




               X_U21.dx        X_U21.dy        
          IS  800.000000E-18  800.000000E-18 
          RS                    1.000000E-03 
         CJO                   10.000000E-12 


               X_U20.x_lm741.dx 
          IS  800.000000E-18 
          RS    1            


               X_U20.x_lm741.dy 
          IS  800.000000E-18 
          RS    1.000000E-03 
         CJO   10.000000E-12 


**** 07/15/05 23:08:00 ********* PSpice 9.2 (Mar 2000) ******** ID# 1 ********

 ** Profile: "SCHEMATIC1-transitoire"  [ D:\workarea\pspice\AOP\integrateur en cascade-SCHEMATIC1-transitoire.sim ] 


 ****     BJT MODEL PARAMETERS


******************************************************************************




               X_U21.qx        X_U20.x_lm741.qx 
               NPN             NPN             
          IS  800.000000E-18  800.000000E-18 
          BF   93.75           93.75         
          NF    1               1            
          BR    1               1            
          NR    1               1            
          CN    2.42            2.42         
           D     .87             .87         


WARNING -- Pulse Period < (Rise Time + Fall Time + Pulse Width) for V_V1

          JOB CONCLUDED

          TOTAL JOB TIME             .11
