
**** 02/15/01 17:15:18 ********* PSpice 9.2 (Mar 2000) ******** ID# 1109000396 
 ** Profile: "SCHEMATIC1-lab3a"  [ D:\ECE 334\Lab4\Lab4\lab4c-schematic1-lab3a.sim ] 


 ****     CIRCUIT DESCRIPTION


******************************************************************************




** Creating circuit file "lab4c-schematic1-lab3a.sim.cir" 
** WARNING: THIS AUTOMATICALLY GENERATED FILE MAY BE OVERWRITTEN BY SUBSEQUENT SIMULATIONS

*Libraries: 
* Local Libraries :
* From [PSPICE NETLIST] section of C:\Program Files\Orcad\PSpice\PSpice.ini file:
.lib "nom.lib" 

*Analysis directives: 
.DC LIN V1 -5 5 0.1 
.PROBE V(*) I(*) W(*) D(*) NOISE(*) 
.INC ".\Lab4C-SCHEMATIC1.net" 



**** INCLUDING Lab4C-SCHEMATIC1.net ****
* source LAB4C
C_C1         N03593 N03252  10n  
V_V3         N02289 0 12Vdc
V_V4         N02283 0 -12Vdc
R_R2         N03987 N03593  10k  
V_V2         N03987 0  
+SIN 0 0.015 1000Hz 0 0 0
X_U8         N03593 0 N02289 N02283 N03252 LM741

**** RESUMING lab4c-schematic1-lab3a.sim.cir ****
.END

ERROR -- DC device V1 is undefined