
**** 07/15/05 21:53:43 ********* PSpice 9.2 (Mar 2000) ******** ID# 1 ********

 ** Profile: "SCHEMATIC1-simple alternance"  [ D:\workarea\pspice\Redressement-doubleur\simple alternance-SCHEMATIC1-simple alternanc


 ****     CIRCUIT DESCRIPTION


******************************************************************************




** Creating circuit file "simple alternance-SCHEMATIC1-simple alternance.sim.cir" 
** WARNING: THIS AUTOMATICALLY GENERATED FILE MAY BE OVERWRITTEN BY SUBSEQUENT SIMULATIONS

*Libraries: 
* Local Libraries :
* From [PSPICE NETLIST] section of D:\Orcad\PSpice\PSpice.ini file:
.lib "nom.lib" 

*Analysis directives: 
.TRAN  0 0.00825 0 
.PROBE V(*) I(*) W(*) D(*) NOISE(*) 
.INC ".\simple alternance-SCHEMATIC1.net" 



**** INCLUDING "simple alternance-SCHEMATIC1.net" ****
* source SIMPLE ALTERNANCE
X_D1         N00231 N00159 D1N5814 
R_R1         0 N00159  10k  
C_C1         0 N00159  100u  
V_V1         N00231 0  
+SIN 0 10V 500Hz 0 0 0

**** RESUMING "simple alternance-SCHEMATIC1-simple alternance.sim.cir" ****
.END

**** 07/15/05 21:53:43 ********* PSpice 9.2 (Mar 2000) ******** ID# 1 ********

 ** Profile: "SCHEMATIC1-simple alternance"  [ D:\workarea\pspice\Redressement-doubleur\simple alternance-SCHEMATIC1-simple alternanc


 ****     Diode MODEL PARAMETERS


******************************************************************************




               X_D1.DFWD       
          IS  344.707200E-09 
           N    1.63162      
         ISR  162.854500E-09 
          NR    1.70788      
         IKF     .113748     
          BV  120.29         
         IBV    6.4502       
          RS    2.706738E-03 
          TT   60.667000E-09 
         CJO  534.450000E-12 
          VJ     .48463      
           M     .40878      


**** 07/15/05 21:53:43 ********* PSpice 9.2 (Mar 2000) ******** ID# 1 ********

 ** Profile: "SCHEMATIC1-simple alternance"  [ D:\workarea\pspice\Redressement-doubleur\simple alternance-SCHEMATIC1-simple alternanc


 ****     INITIAL TRANSIENT SOLUTION       TEMPERATURE =   27.000 DEG C


******************************************************************************



 NODE   VOLTAGE     NODE   VOLTAGE     NODE   VOLTAGE     NODE   VOLTAGE


(N00159)-425.5E-21 (N00231)    0.0000 




    VOLTAGE SOURCE CURRENTS
    NAME         CURRENT

    V_V1         4.255E-23

    TOTAL POWER DISSIPATION   0.00E+00  WATTS



          JOB CONCLUDED

          TOTAL JOB TIME             .05
