OSU Standard Cell Libaray

Supported Technologies
AMI 0.5um -> ami05
AMI 0.35um -> ami035
TSMC 0.25um -> tsmc025
TSMC 0.18um -> tsmc018

Directory structure
-------------------
./tsmc018/osu_stdcells_tsmc018	DFII Library for Cadence ICFB
         /abstract		Abstract run directory to create lef file
         /signalstorm		Signalstorm run directory for all timing files
         /html			HTML cell documentation
         /lib			Container folder for all library files

Similarly for the other 3 technologies.

./source/gds2			GDS streams of all cell libraries
        /magic			Magic layout of all cells
        /magic.abstract		Magic layouts with pin names
	/pads_ami05		Magic layouts for AMI 0.5 pads
	/pads_ami035		Magic layouts for AMI 0.35 pads
	/sue			Sue schematics for AMI 0.5
	/osu_stdcells.area	Area in lambda-square for all cells

Note for AMI 0.5um
------------------
osu05_stdcells.lef		Lef file without stacked vias
osu05_stdcells.stacks.lef	Lef file with stacked vias

Both files are valid for Mosis. The file without stacked
vias is provided for Magic 6.5, which doesn't support
stacked vias. The stacked vias file can be used for
Cadence Virtuoso and Magic 7.3.

-------------
Johannes Grad
jgrad@ece.iit.edu
